{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Reclamación","Proceso de trabajo","Circuito Aire Comprimido","Filtros Interior Cabina"],"not_rendered":{"charts":0,"images":14,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Reclamación","index":0,"n_rows":46,"n_cols":4,"rows_kept":46,"cut":false,"hidden":false,"merged":[[13,2,27,4],[29,2,43,4],[45,2,59,4],[1,0,2,4]]}
[]
["Protocolo Reclamación Delaminaciones"]
[]
[]
["Nombre de taller",null,null,"Matrícula"]
["Persona contacto",null,null,"Marca/Coche"]
["Email",null,null,"Modelo"]
["Teléfono",null,null,"Código de color"]
[]
["Responsable PPG",null,null,"Nº Reparación"]
["Fecha reclamación",null,null,"Fecha reparación"]
[]
[]
[null,null,"\nObservaciones:\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"\nObservaciones:\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"\nObservaciones:\n"]

{"sheet":"Proceso de trabajo","index":1,"n_rows":42,"n_cols":3,"rows_kept":42,"cut":false,"hidden":false,"merged":[[2,0,2,2],[16,0,16,2],[0,0,0,2],[31,0,31,2]]}
["PROCESO DE TRABAJO"]
[]
["Preparación Aparejo"]
["Producto","Referencia","Ratio"]
["Aparejo"]
["Catalizador"]
["Diluyente"]
["Proceso de Secado","Minutos","Temperatura"]
["Elige"]
["Proceso Lijado"]
["Orbita","Elige"]
["Grano lija final","Elige"]
["Limpieza (desengrasado)","Elige"]
["Referencia"]
["Escala de Grises utilizada"]
[]
["Preparación Color"]
["Nombre del color"]
["Codigo OEM",{"$f":"+IF(Reclamación!E8=\"\",\"\",Reclamación!E8)","v":""}]
["Tipo de acabado","Elige"]
["Producto","Referencia","Ratio (%)"]
["Color",null,1]
["Aditivo altas prestaciones",null,"Elige"]
["Diluyente",null,"Elige"]
["Proceso Aplicación"]
["Sistema","Elige"]
["Mano de control","Elige"]
["Proceso evaporación","Minutos","Temperatura"]
["Elige"]
[]
[]
["Preparación Barniz"]
["Producto","Referencia","Ratio"]
["Barniz"]
["Catalizador"]
["Diluyente"]
["Proceso Aplicación"]
["Sistema","Elige"]
["Proceso evaporación","Minutos","Temperatura"]
["Elige"]
["Proceso de Secado","Minutos","Temperatura"]
["Elige"]

{"sheet":"Circuito Aire Comprimido","index":2,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[[11,0,11,2],[16,2,18,2],[7,2,9,2],[0,0,0,2],[2,0,2,2],[4,0,4,2],[15,0,15,2]]}
["CIRCUITO AIRE COMPRIMIDO"]
[]
["Revisión Visual"]
[]
["Compresor (Filtro)"]
[]
["Ejemplo Imagen Equipo correcto a revisar","Imagen equipo actual instalación","Imágenes de errores comunes"]
[]
["Elementos cuarto de compresor","Solo compresor"]
["Filtro/s","Elige"]
[]
["Red (Manchas canalización)"]
[]
["Estado conexiones canalización","Se aprecian manchas"]
[]
["Refrigerador - secador"]
[]
["Estado Secador","Funciona"]
["Estado Refrigerador","Funciona"]

{"sheet":"Filtros Interior Cabina","index":3,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[[19,0,19,4],[13,2,16,2],[12,0,12,4],[13,0,16,0],[0,0,0,4],[4,0,4,1],[6,0,6,1],[7,0,7,1],[9,0,9,1],[2,0,2,4],[8,0,8,1]]}
["Filtros interior cabina"]
[]
["Revisión Visual"]
[null,null,"Imagen Equipo correcto a revisar","Imagen actual instalación","Atención - errores comunes"]
["Filtros interior cabina "]
[]
["Filtros instalados",null,"para particulas y coalescentes"]
["Estado exterior",null,"Manchados (no pintura)"]
["Mantenimiento",null,"Revisados"]
["Fecha Última revisión",null,"2018-12-05"]
[]
[]
["Medición Calidad Aire (EQUIPO)"]
[null,null,null,"Partículas","Aparecen"]
[null,null,null,"Aceite Agua","No aparecen"]
[null,null,null,"Temperatura ",25]
[null,null,null,"Humedad relativa (%)",0.23]
[]
[]
["Interior del filtro"]
["Comprobación cuerpos Filtrado","Estado","Imagen Equipo correcto a revisar","Imagen actual instalación","Ejemplo equipo contaminado "]
["Agua + Partículas","Elige"]
["Agua/Aceite (coalescente)","Elige"]
["Carbon activo","Elige"]